// Schedule TX every this many seconds (might become longer due to duty

// cycle limitations).

const unsigned TX\_INTERVAL = 20;

// Pin mapping

const lmic\_pinmap lmic\_pins = {

.nss = 10,// Connected to pin D10

.rxtx = LMIC\_UNUSED\_PIN,// For placeholder only, Do not connected on RFM92/RFM95

.rst = 9,// Needed on RFM92/RFM95? (probably not)

.dio = {5, 6, 7},// Specify pin numbers for DIO0, 1, 2

};